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RST® connection cable IP66/68(3 m; 2 h)/69, male, free end, 3x 1.5 mm², 250 V, 16 A, B2ca, length: 3 m, black

System RST® MINI - assembled H05VV-F connection cable IP66/68(3 m; 2 h)/69, 3-pole, 1.5 mm², fire class B2ca, with locking, male RST16i3, free end (ultrasonic welded), according to IEC 61535, mechanical coding light gray/black, color coding black.

Rated voltage: 250 V
Rated current: 16 A
Rated impulse voltage: 4 kV
Type of protection: IP66/68(3 m; 2 h)/69
Cable type: H05VV-F
Fire class: B2ca
Cable color: black
Halogen-free: yes
Length: 3 m

Brand: Wieland Electric GmbH  
Type: RST16I3K1S 15B 30SW
Part No.: 46.432.30B4.1

