
RST® MINI MOLA Device connector M20 with contact seal, IP66/68(3 m; 2 h)/69, male, 5-pole, 250 / 400 V, 16 A, black

System RST® MINI MOLA - Device connector according to IEC 61535 for permanent installation, self-locking, with contact seal, for simplified or automated internal wiring of luminaires or similar devices, due to the modular design the housing and internal ballast can be wired independently of each other and can be brought together later, male, 5-pole, turned contacts with push-in spring, fastening screw from inside, mechanical coding light gray/black, color coding black.

Rated voltage: 250 / 400 V
Rated current: 16 A
Rated impulse voltage: 4 kV
Type of protection: IP66/68(3 m; 2 h)/69
Diameter/thread: M20
Wall thicknesses: up to 4 mm
Rated cross-section connecting-channel A: 1.0 – 2.5 mm² (with ferrules up to 1.5 mm²)
Rated cross-section connecting-channel B (solid): 0.5 – 1.0 mm²
Rated cross-section connecting-channel B (fine stranded): 0.75 – 1.0 mm²
Rated cross-section connecting-channel B (ferrules): 0.5 mm²
Housing material: PA66, V2
Sealing material: NBR
Connections per pole: 2
Marking: 1, 2, 3, N, PE
Contact seal per pole: yes
Halogen-free: yes

Brand: Wieland Electric GmbH
Type: RST16I5 2 D03 MSW
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