
podis® CON Feed-In and Tap-Off module FCS 16 5 SI SA M32

System podis® CON - Feed-In and Tap-Off module for flat cable 5G16; for fixed wiring as feed-in or tap-off; for M32 cable gland; 5-pole; ratings acc. to VDE 63 A; 690 V; 6kV/3; ratings acc. to UL 32 A; 600 V; degree of protection IP65; piercing contacts; Torx 15; screw terminals max. 16 mm² (AWG 6) single/fine-stranded; max. cable diameter 25 mm; housing black; mounting position any; outline dimensions 250x84x74 mm (LxWxH)

Rated voltage: 690 V
Rated current: 63 A
Color: black
Material: metal, plastic

Brand: Wieland Electric GmbH
Type: FCS 16 5 SI SA M32
Part No.: 75.456.0053.1 
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