
gesis® WIV Distribution Box 20 kVA with RST® POWER, gesis® CLASSIC 12/1/2/0/2

System gesis® WIV – Pre-wired system distributor with pluggable infeed via an RST50 or 32 A CEKON three-phase power supply for a maximum connected load of 20 kVA. The outputs are provided via the GST18® installation coupler system approved in accordance with IEC 61535. Each circuit is individually fused, the 16 A outlets are FI-protected. Several connections can be switched on or off via a common main switch. The distribution system consists of switchable and non-switchable outlets. If required, the non-switchable outlets can be used to operate e.g. emergency lighting or cooling systems. They are also suitable for extending existing installations and are easy to put into operation. An adapter cable 3 m, 32 A CEKON to RST50 is included in delivery.

Connected load: 20 kVA
Maximum fuse: 32 A
Connection type infeed: pluggable RST50
Pluggable system outputs: GST18® and safety sockets
Total output power: 20 kVA
Switchable 1-phase outputs: 12
Switchable 3-phase outputs: 1
Non-switchable 1-phase outputs: 2
Safety socket: 2
Residual current circuit breaker, 4-pole, 40 A, 30 mA: 1
Miniature circuit breaker, 1-pole, B, 16 A: 14
Miniature circuit breaker, 3-pole, B, 16 A: 1
Main switch 63 A: 1 
Housing material: polycarbonate
Housing color: electric grey 
Ambient conditions: for dry rooms only
Protection class without mating connectors: IP20
Protection class all mating connectors connected: IP40 
Mounting method: wall mounting
Depth: 155 mm
Width: 315 mm 
Height: 630 mm

Brand: Wieland Electric GmbH
Type: WIV 20 P GC 12-1-2-0-2
Part No.: 93.053.6009.0 
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