
gesis® SPZ Distribution box with integrated RCBO C16 A 4-pole in increased protection class

System gesis® SPZ - Distribution box, pre-wired for pluggable decentralized fuse protection for EVC applications. In the sealable housing made of plastic a 5-pole RST® CLASSIC (Type: RST25i5), concrete grey coded, offers the possibility of a pluggable input. Internally, a 4-pole RCBO type A with tripping characteristic C16 A /30 mA is installed and wired. The output is designed as a pluggable RST® CLASSIC 5-pole (Type: RST25i5), concrete grey coded. 

Connection type inputs: RST® CLASSIC (RST25i5)
Colour coding of the input: concrete grey
3-phase inputs: 1
Fuse protection: RCBO C16 A / 0,03 A, Type A
Plug-in system outputs: RST® CLASSIC (RST25i5)
3-phase outputs: 1
Colour coding of the output: concrete grey
Enclosure material: others
Protection class: IP65
Mounting type: wall, floor, ceiling 
Length: 143 mm
Width: 210 mm
Height: 100 mm

Make: Wieland Electric GmbH
Type: SPZ 4P-FI-C16-A-R25-1/1
Part No.: 98.554.1200.6 
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