
gesis® SPZ Distribution box as kit with RST25i5 input/output in increased protection class

System gesis® SPZ - Distribution box, prepared kit for pluggable decentralized protection of EVC applications. In the sealable housing made of plastic with a width of 4 DU a 5-pole RST® CLASSIC (Type: RST25i5), concrete grey coded, offers the possibility of a pluggable input. Internally, a DIN rail is mounted, which can be used for the installation of protection/switching devices. The output is designed as a pluggable RST® CLASSIC 5-pole (Type: RST25i5), concrete grey coded. 

Connection type inputs: RST® CLASSIC (RST25i5)
Colour coding of the input: concrete grey
3-phase inputs: 1
DIN rail integrated: yes
Plug-in system outputs: RST® CLASSIC (RST25i5)
3-phase outputs: 1
Colour coding of the output: concrete grey
Enclosure material: others
Protection class: IP65
Mounting type: wall, floor, ceiling 
Length: 143 mm
Width: 210 mm
Height: 100 mm

Make: Wieland Electric GmbH
Type: SPZ EVC Bausatz R25-1/1
Part No.: 98.554.1200.0 
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