
podis® CON Connection module, 5G6 mm², M25, IP65, 690 V, 20 A, black

System podis® CON - Connection module 5G6 connection via round cable; M25 cable gland; 5-pole; nominal ratings acc. VDE 20 A; 690 V; 6kV/3; nominal ratings acc. UL 32 A; 600 V degree of protection IP65; piercing contacts; Torx 15; screw clamps max. 16 mm² single/fine stranded; max. Cable diameter 18 mm; housing black; mounting position any; outline dimensions 245x84x59 mm (LxWxH).

Rated voltage: 690 V
Rated current: 20 A
No. of Poles: 5
Degree of protection: IP65
Cross-Section: 6 mm²
Cable diameter: 9 - 18 mm
Halogen-free: yes
Color: black

Brand: Wieland Electric GmbH
Type: FCS 6 5 SI SA M25 LH
Part No.: 75.256.0153.1 
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