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podis® CON Connection module, 5G6 mm², M32, IP65, 690 V, 41 A, black

System podis® CON - Connection module 5G6 connection via round cable; M32 cable gland; 5-pole; nominal ratings acc. VDE 41 A; 690 V; 6kV/3; nominal ratings acc. UL 32 A; 600 V; degree of protection IP65; piercing contacts; Torx 15; screw clamps max. 16 mm² single-/fine stranded; max. cable diameter 25 mm; housing black; mounting position any; outline dimensions 250x84x74 mm (LxWxH).

Rated voltage: 690 V
Rated current: 41 A
No. of Poles: 5
Degree of protection: IP65
Cross-Section: 6 mm²
Cable diameter: 10 - 25 mm
Halogen-free: yes
Color: black

Brand: Wieland Electric GmbH 
Type: FCS 6 5 SI SA M32
Part No.: 75.250.0053.1 
[bookmark: _GoBack]

