
podis® CON Flat cable, 5G6 mm², 0.6/1 kV, black, halogen free

System podis® CON - Flat cable XPE 5G6; 0,6/1kV; Approval acc. CE, UL 1277 TC-ER 32 A, 600 V; ampacity IEC acc. VDE 0298-4 tables 5 and 6; fine-stranded, halogen free; for fixed installation; color black; 43x7.8 mm (WxH).

Rated voltage: 0.6/1 kV
Cable color: black
Fire behavior: self-extinguishing according to IEC 60332-1-2
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: XPE 5G6 black
Part No.: 00.729.0305.1 
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