
podis® CON PLC module, 5G16, IP65, LS 10 kA 1+N, C13 A, black

System podis® CON - PLC-Module Tap-Off; with facility for the integration of rail-mounted devices (4 modular spacing); included is a MCB 10 kA, 1+N with tripping characteristic C13 A including the wiring and a separable cable gland for the communication cable (RJ45); for M32 cable gland output, plus optional knock-outs for M20 cable gland and M12; lockable with padlock; color black

Rated voltage: 230 V
Rated current: 13 A
No. of Poles: 5
Degree of protection: IP65
Halogen-free: yes
Color: black

Brand: Wieland Electric GmbH
Type: PLC MODUL ADAPTER
Part No.: G0.000.0157.0 
[bookmark: _GoBack]

