
podis® CON Flat cable, 5G25 mm², 0.6/1 kV, B2ca s1a d1 a1, grey, halogen-free

System podis® CON - Flat cable LSHF 5G25; 0.6/1kV; CPR class B2ca s1a d1 a1; halogen-free, flame retardant; for fixed installation; color grey; Rated Current: 63 A; 48x11.5 mm (WxH)

Rated voltage: 0.6/1 kV
Cable color: grey
Insulation material: polyolefin
Fire behavior: self-extinguishing according to IEC 60332-1-2
Fire class: B2ca s1a d1 a1
Halogen-free: yes

Brand: Wieland Electric GmbH
Type: LSHF 5G25
Part No.: 99.099.0000.8 


podis® CON Connection module, 5G16 mm², RST20i5, IP65, 400 V, 20 A black

System podis® CON - Connection module 5G16 RST for pluggable connection with RST20i5; 5-pole; nominal ratings acc. VDE 20 A; 400 V; nominal ratings acc. UL 20 A; 600 V; degree of protection IP65; piercing contacts; Torx 15; housing black; mounting position any; outline dimensions 217x84x74 mm (LxWxH).

Rated voltage: 400 V
Rated current: 20 A
No. of Poles: 5
Degree of protection: IP65
Halogen-free: yes
Color: black

Brand: Wieland Electric GmbH 
Type: FCS 16 5 SI SA RST
Part No.: 75.452.0053.1 
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