
podis® CON Circuit breaker module, 5G16, RST20i5, IP65, RCBO type A C16 A / 30 mA, black

System podis® CON - Circuit breaker module; combines tap-off and decentralized fuse-protection; internally, a 4-pole RCBO type A with tripping characteristic C16 A /30 mA is installed and wired; with an integrated pluggable output RST20i5 in black; lockable with padlock; color black

Rated voltage: 400 V
Rated current: 16 A
No. of Poles: 5
Degree of protection: IP65
Cross-Section: 2.5 mm²
Cable diameter: 10 – 25 mm
Halogen-free: yes
Color: black 

Brand: Wieland Electric GmbH
Type: FH RCBO 16 CARST20
Part No.: 75.456.1155.1 
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