
podis® CON Circuit breaker module, 5G16, M32, IP65, for self-assembly, black

System podis® CON - Circuit breaker module; combines tap-off and decentralized fuse-protection; with facility for the integration of rail-mounted devices (4 modular spacing); for M32 cable gland output, plus optional knock-outs for M20 cable gland and M12; lockable with padlock; color black

Rated voltage: 690 V
Rated current: 63 A
No. of Poles: 5
Degree of protection: IP65
Cable diameter: 10 – 25 mm
Halogen-free: yes
Color: black

Brand: Wieland Electric GmbH
Type: FH MT        M32
Part No.: 75.456.1055.1 
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