
podis® CON Feed-in- and tap-off module, 5G16, M32, IP65, black

System podis® CON – Connection module (high version) for fixed wiring, as
feed-in or tap- off; for M32 cable gland; 5- pole; nominal ratings acc. VDE 63 A; 690 V; 6kV/3; degree of protection IP65; piercing contacts; Torx 15; screw clamps max. 16 mm² (AWG 6) single/fine- stranded; max. cable diameter 25 mm; housing black; mounting position any; Outline dimensions 219x147x84 mm (LxBxH)

Rated voltage: 690 V
Rated current: 63 A
No. of Poles: 5
Degree of protection: IP65
Cross-Section: 16 mm²
Cable diameter: 10 – 25 mm
Halogen-free: yes
Color: black

Brand: Wieland Electric GmbH
Type: FCS 16 5 SI SA M32 XF
Part No.: 75.456.0753.1 
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