
podis® CON Circuit breaker module, 5G16, RST25i5, IP65, LS C32 A / 30 mA, black

System podis® CON - Circuit breaker module; combines tap-off and decentralized fuse-protection; internally, a 4-pole MCB with tripping characteristic C32 A is installed and wired; with an integrated pluggable output RST25i5 in concrete gray; lockable with padlock; color black

Rated voltage: 400 V
Rated current: 32 A
No. of Poles: 5
Degree of protection: IP65
Cross-Section: 6 mm²
Halogen-free: yes
Color: black 

Brand: Wieland Electric GmbH
Type: FH  BO  32 C RST25
Part No.: 75.453.1755.1 
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