
podis® CON Connection module double output, 5G16, RST25, IP65, black

System podis® CON – Connection module (high version) with double output podis CON 5G16 for
pluggable connection with RST25i5; 5-pole; Rated current module 63 A; operating current per output up to 32 A acc. VDE / IEC 61984 derating curve of RST25i5 System; Rated voltage 400 V; degree of protection IP65; piercing contacts; Torx 15; housing black; mounting position any; outline dimensions 218x84x146 mm (LxWxH)

Rated voltage: 400 V
Rated current: 63 A
No. of Poles: 5
Degree of protection: IP65
Cross-Section: 6 mm²
Cable diameter: 10 – 25 mm
Halogen-free: yes
Color: black

Brand: Wieland Electric GmbH
Type: FCS 16 5 SI SA RST25
Part No.: 75.453.0353.1 
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