
podis® CON Feed-in module, 5G16, IP65, 690V, 100 A, grey

System podis® CON – Feed-in module for flat cable 5G16; connection by roundcable; cut-out for entry of the round cable with a diameter of 25 mm; 5-pole; nominal ratings acc. IEC 100 A; 690 V; 6kV/3; nominal ratings acc. UL 61 A; 600 V; degree of protection IP65; screw clamps max. 35 mm² (AWG 2) single/fine-stranded; (1 ½"); housing grey; mounting position any; Outline dimensions 300x145x100 mm (LxWxH)

Rated voltage: 690 V
Rated current: 100 A
No. of Poles: 5
Degree of protection: IP65
Cross-Section Flat cable: 16 mm²
Halogen-free: yes
Color: grey

Brand: Wieland Electric GmbH
Type: FCS  16  5 SA SAM
Part No.: 75.450.2114.3 
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