
podis® CON Flat cable, 5G16 mm², 0.6/1 kV, B2ca s1a d1 a1, grey white, halogen-free

System podis® CON - Flat cable LSHF 5G16; 0.6/1kV; CPR class B2ca s1a d1 a1; Ampacity up to 63 A; halogen-free; flame retardant; for fixed installation; color grey white; 48x11.5 mm (WxH)

Rated voltage: 0.6/1 kV
Cable color: grey-white
Insulation material: polyolefin
Fire behavior: self-extinguishing according to IEC 60332-1-2
Fire class: B2ca s1a d1 a1
Halogen-free: yes

Brand: Wieland Electric GmbH
Type: LSHF 5G16
Part No.: 00.771.0307.3 
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