
RST® circular connector, IP66/67/69K, male, 4-pole, 250/400 V, 50 A

System RST® POWER - Circular connector with type of protection IP66/67/69K, male, 4-pole, turned contacts with screw connection compact housing with strain relief, field assembly, mechanical/color coding black.

Rated voltage: 250/400 V
Rated current: 50 A
Rated impulse voltage: 4 kV
Type of protection: up to IP66/67/69K
Terminal cross-section (solid/stranded): 4.0 - 6.0 mm²
Terminal cross-section (flexible wires): 4.0 - 16.0 mm²
Cable diameter: 20 - 32 mm
Cable gland: M40
Housing material: PA66, V2
Sealing material: NBR
Connections per pole: 1
Marking: PE, 1, 2, 3
Halogen-free: yes

Brand: Wieland Electric GmbH
Type: RST50I4S S1 ZR6 S SW
Part No.: 97.042.4253.1
[bookmark: _GoBack]

