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gesis® extension cable, female, male, 2x 0.5 mm², shed, 50 V, 3 A, Dca, length: 1 m, black

System gesis® NV - assembled FB-H(St) 2x210.8 extension cable, 3-pole, 0.5 mm², fire class Dca, male BST14i3, female BST14i3, mechanical coding code 3, color coding black.

Rated voltage: 50 V
Rated current: 3 A
Type of protection: IP20
Cable type: FB-H(St) 2x210.8
Fire class: Dca
Cable color: green
Halogen-free: yes
Length: 1 m

Brand: Wieland Electric GmbH 
Type: BST14i3 KF BS 50H 10SW
Part No.: 94.435.1060.1

