
gesis® extension cable, female, male, 2x 0.5 mm², 50 V, 3 A, Dca, length: 3 m, black

System gesis® NV - assembled FB-H(St) 2x2x0.8 extension cable, 2-pole, 0.5 mm², fire class Eca, male BST14i2, female BST14i2, mechanical coding code 2, color coding pastel blue.

Rated voltage: 50 V
Rated current: 3 A
Type of protection: IP20
Cable type: FB-H(St) 2x2x0.8
Fire class: Eca
Cable color: black
Halogen-free: yes
Length: 3 m

Brand: Wieland Electric GmbH 
Type: BST14i2 KF BS 50Z 30PB02
Part No.: 94.425.3060.9 
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