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gesis® extension cable, female, male, 2x 0.5 mm², 50 V, 3 A, Dca, length: 3 m, green

System gesis® NV - assembled FB-H(St) 2x230.8 extension cable, 2-pole, 0.5 mm², ², fire class Dca, male BST14i2, female BST14i2, mechanical coding code 1, color coding green.

Rated voltage: 50 V
Rated current: 3 A
Type of protection: IP20
Approval: KNX certified
Cable type: FB-H(St) 2x230.8
Fire class: Dca
Cable color: green
Halogen-free: yes
Length: 3 m

Brand: Wieland Electric GmbH 
Type: BST14i2 KF BS 50H 30GN01
Part No.: 94.425.3060.7

