[bookmark: _GoBack]
gesis® connection cable, male, free end, 2x 0.5 mm², 50 V, 3 A, Eca, length: 1 m, black

System gesis® NV - assembled L03Z1Z1-U connection cable, 2-pole, 0.5 mm², fire class Eca, male BST14i2, free end, mechanical coding code 2, color coding pastel blue.

Rated voltage: 50 V
Rated current: 3 A
Type of protection: IP20
Cable type: L03Z1Z1-U
Fire class: Eca
Cable color: black
Halogen-free: yes
Length: 1 m

Brand: Wieland Electric GmbH 
Type: BST14i2 KF -S 50Z 10PB02
Part No.: 94.425.1094.9

