
gesis® connector, male, 3-pole, 50 V, 3 A, black 

System gesis® NV - Connectors for bus/signal cables (e.g. LON), male version, 3-pole, with spring clamp connection, compact housing with strain relief and locking, field assembly, mechanical coding code 3, color coding black.

Rated voltage: 50 V
Rated current: 3 A
Type of protection: IP20
Terminal cross-section, solid: 0.25 - 0.75 mm²
Terminal cross-section, stranded: 0.25 - 0.75 mm²
Cable diameter: 5.5 - 6.5 mm
Housing material: Polyamide
Connections per pole: 1
Marking: 2-, 1+
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: BST14i3 F S1 Z R1 MSW
Part No.: 93.432.2553.1
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