
gesis® Snap-In, female, 3-pole, for panel mounting, 50 V, 3 A, black

System gesis® NV - Connectors for bus/signal cables (e.g. LON), female version, 3-pole, with spring clamp connection, snapable in housing, with integrated locking, mechanical coding code 3, color coding black.

Rated voltage: 50 V
Rated current: 3 A
Type of protection: IP20
Terminal cross-section, solid: 0.25 - 0.75 mm²
Terminal cross-section, stranded: 0.25 - 0.75 mm²
Housing material: Polyamide
Connections per pole: 1
Marking: 1+, 2-
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: BST14i3 F B1 R SW
Part No.: 93.431.2353.1
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