
gesis® distribution block, 2-pole, 1 input, 2 outputs, 50 V, 3 A, pastel blue

System gesis® NV - Distribution blocks for bus/signal cables, T-shaped distribution block, 2-pole, 1 input, 2 outputs, with integrated locking, mechanical coding code 2, color coding pastel blue.

Rated voltage: 50 V
Rated current: 3 A
Type of protection: IP20
Housing material: Polyamide
Input: 1
Outputs: 2
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: BST14i2 V 2P1 T PB02 
Part No.: 93.420.4653.0
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