
gesis® Snap-In, male, 5-pole, for panel mounting, 250/400 V, 16 A, black

System gesis® MINI - Installation connector according to IEC 61535 for permanent connection, male version, 5-pole, turned contacts with screw connection, with white frame, snapable in housing, with integrated locking, mechanical coding code 1, color coding black.

Rated voltage: 250/400 V
Rated current: 16 A
Rated impulse voltage: 4 kV
Type of protection: up to IP40
Material thickness: 0.5 - 1.5 mm
Terminal cross-section, solid: 0.5 - 2.5 mm²
Terminal cross-section, stranded: 0.5 - 2.5 mm²
Housing material: Polyamide
Connections per pole: 1
Marking: 3, 2, 1, PE, N
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: GST15i5S S1 R V SW
Part No.: 91.952.9053.1
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