
gesis® connector, female, 4-pole, 250/400 V, 16 A, white 

System gesis® MINI - Installation connector according to IEC 61535 for permanent connection, female version, 4-pole, 5-pole housing, turned contacts with screw connection, very compact housing with strain relief, field assembly, mechanical coding code 1, color coding white.

Rated voltage: 250/400 V
Rated current: 16 A
Rated impulse voltage: 4 kV
Type of protection: up to IP40
Terminal cross-section, solid: 0.5 - 2.5 mm²
Terminal cross-section, stranded: 0.5 - 2.5 mm²
Cable diameter: 8.5 - 12.5 mm (H05VV-F, NYM)
Housing material: Polyamide
Connections per pole: 1
Marking: N, PE, 1, 2
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: GST15i4 S B1 Z R1 WS
Part No.: 91.941.4053.0
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