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gesis® extension cable, female, male, 5x 1.5 mm², 250/400 V, 16 A, Eca, length: 2 m, black

System gesis® MINI - assembled H05VV-F extension cable with protective ground, 5-pole, 1.5 mm², fire class Eca, male GST15i5, female GST15i5, with angled cable entry, according IEC 61535, mechanical coding code 1, color coding black.

Rated voltage: 250/400 V
Rated current: 16 A
Rated impulse voltage: 4 kV
Type of protection (plugged): IP40
Type of protection (unplugged): IP20
Cable type: H05VV-F
Fire class: Eca
Cable color: black
Halogen-free: no
Length: 2 m

Brand: Wieland Electric GmbH 
Type: GST15i5KS BS X15 V 20SW
Part No.: 91.257.2000.1

