
gesis® intermediate coupling, 5-pole, 1 input, 1 output, 250 V, 16 A, white

System gesis® MINI - Intermediate coupling for installation connectors according to IEC 61535, for direct forwarding e.g. between two luminaires, 5-pole, turned contacts, 1 input, 1 output, mechanical coding code 1, color coding white.

Rated voltage: 250/400 V
Rated current: 16 A
Rated impulse voltage: 4 kV
Type of protection (plugged): IP40
Type of protection (unplugged): IP20
Housing material: Polyamide
Input: 1
Output: 1
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: GST15i5 Z 1P1 WS
Part No.: 91.050.5953.0
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