
gesis® connector, male, 5-pole, 250/400 V, 20 A, black 

System gesis® CLASSIC - Installation connector according to IEC 61535 for permanent connection, male version, 5-pole, turned contacts with screw connection, compact housing with strain relief, field assembly, mechanical coding code 1, color coding black.

Rated voltage: 250/400 V
Rated current: 20 A
Rated impulse voltage: 4 kV
Type of protection: IP40
Terminal cross-section, solid: 0.75 - 2.5 mm²
Terminal cross-section, stranded: 0.75 - 2.5 mm²
Cable diameter: 7 - 13.5 mm (H05VV, NYM)
Housing material: Polyamide
Connections per pole: 1
Marking: 1, 2, PE, N, 3
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: GST18i5 S S1 Z R1 SW
Part No.: 92.954.4053.1
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