
gesis® connector with test tap, female, 5-pole, 250 V, 20 A, pastel blue 

System gesis® CLASSIC - Installation connector according to IEC 61535 for permanent connection, for dimming applications, female version with test tap, 5-pole, turned contacts with screw connection, compact housing with strain relief, field assembly, mechanical coding code 2, color coding pastel blue.

Rated voltage: 250 V
Rated current: 20 A
Rated impulse voltage: 4 kV
Type of protection: IP40
Terminal cross-section, solid: 0.5 - 4 mm²
Terminal cross-section, stranded: 0.5 - 4 mm²
Cable diameter: 11.5 - 15.5 mm (H05VV, NYM)
Housing material: Polyamide
Connections per pole: 1
Marking: L, N, PE, D2, D1
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: GST18i5 S B1 Z R1 PB02
Part No.: 92.953.7453.0
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