
gesis® connector, male, 4-pole, 250/400 V, 20 A, white 

System gesis® CLASSIC - Installation connector according to IEC 61535 for permanent connection, male version, 4-pole, turned contacts with spring clamp connection, compact housing with strain relief, field assembly, mechanical coding code 1, color coding white.

Rated voltage: 250/400 V
Rated current: 20 A
Rated impulse voltage: 4 kV
Type of protection: IP40
Terminal cross-section, solid: 1.5 - 2.5 mm²
Terminal cross-section, stranded: 1.5 mm² with ferrule
Cable diameter: 9.5 - 11.5 mm (H05VV, NYM, H05RNF)
Housing material: Polyamide
Connections per pole: 2
Marking: 1, PE, N, 2
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: GST18i4 F S2 Z R1 WS
Part No.: 92.944.0053.0
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