
gesis® connector, female, 4-pole, 250/400 V, 20 A, tomato red

System gesis® CLASSIC - Installation connector according to IEC 61535 for permanent connection, female version, 4-pole, turned contacts with screw connection, compact housing with strain relief, field assembly, mechanical coding code 2, color coding tomato red.

Rated voltage: 250/400 V
Rated current: 20 A
Rated impulse voltage: 4 kV
Type of protection: IP40
Terminal cross-section, solid: 0.75 - 2.5 mm²
Terminal cross-section, stranded: 0.75 - 2.5 mm²
Cable diameter: 7.1 - 12.0 mm (H05VV, NYM)
Housing material: Polyamide
Connections per pole: 1
Marking: 2, N, PE, 1
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: GST18i4 S B1 Z R1 TR01
Part No.: 92.943.3553.5
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