
gesis® connector, female, 4-pole, 250/400 V, 20 A, may green

System gesis® CLASSIC - Installation connector according to IEC 61535 for permanent connection, female version, 4-pole, turned contacts with spring clamp connection, compact housing with strain relief, field assembly, mechanical coding code 4, color coding may green.

Rated voltage: 250/400 V
Rated current: 20 A
Rated impulse voltage: 4 kV
Type of protection: IP40
Terminal cross-section, solid: 1.5 - 2.5 mm²
Terminal cross-section, stranded: 1.5 mm² with ferrule
Cable diameter: 9.5 - 11.5 mm (H05VV, NYM, H05RNF)
Housing material: Polyamide
Connections per pole: 2
Marking: 3, 2/N, PE, 1
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: GST18i4 F B2 Z R1 GN02
Part No.: 92.943.0353.0
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