
gesis® connector, female, 3-pole, 250 V, 20 A, brown 

System gesis® CLASSIC - Installation connector according to IEC 61535 for permanent connection, female version, 3-pole, turned contacts with spring clamp connection, compact housing with strain relief, field assembly, mechanical coding code 4, color coding brown.

Rated voltage: 250 V
Rated current: 20 A
Rated impulse voltage: 4 kV
Type of protection: IP40
Terminal cross-section, solid: 1.5 - 2.5 mm²
Terminal cross-section, stranded: 1.5 mm² with ferrule
Cable diameter: 7.8 - 10.3 mm (H05VV, NYM)
Housing material: Polyamide
Connections per pole: 2
Marking: 3, 2, 1
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: GST18i3 F B2 Z R1 BR05
Part No.: 92.933.0453.0
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