
gesis® connector, male, 3-pole, 250 V, 20 A, 4 mm², black 

System gesis® CLASSIC - Installation connector according to IEC 61535 for permanent connection, male version, 3-pole, turned contacts with screw connection, for terminal cross-sections up to 4 mm², compact housing with strain relief, field assembly, mechanical coding code 1, color coding black.

Rated voltage: 250 V
Rated current: 20 A
Rated impulse voltage: 4 kV
Type of protection: IP40
Terminal cross-section, solid: 0.75 - 4 mm²
Terminal cross-section, stranded: 0.5 - 4 mm²
Cable diameter: 10.5 - 14.5 mm (H05VV, NYM)
Housing material: Polyamide
Connections per pole: 1
Marking: L, PE, N
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: GST18i3 S S1 Z R2 SW
Part No.: 92.932.5053.1
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