
gesis® connector, male, 3-pole, 250 V, 20 A, light ivory

System gesis® CLASSIC - Installation connector according to IEC 61535 for permanent connection, especially for applications requiring fire hazard tests as per the standard EN 60335-1, male version, 3-pole, turned contacts with screw connection, compact housing with strain relief, field assembly, mechanical coding code 1, color coding light ivory.

Rated voltage: 250 V
Rated current: 20 A
Rated impulse voltage: 4 kV
Type of protection: IP40
Terminal cross-section, solid: 0.75 - 2.5 mm²
Terminal cross-section, stranded: 0.75 - 2.5 mm²
Cable diameter: 6.5 - 10.5 mm
Housing material: Polyamide
Connections per pole: 1
Marking: L, PE, N
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: GST18i3 S S1 Z R1 N
Part No.: 92.932.3057.0
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