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gesis® connection cable, male, free end, 3x 1.5 mm², 250 V, 16 A, Eca, length: 5 m, may green
System gesis® CLASSIC - assembled H05Z1Z1-F connection cable with protective ground, 3-pole, 1.5 mm², fire class Eca, male GST18i3, free end (ultrasonic welded), according IEC 61535, mechanical coding code 7, color coding may green.

Rated voltage: 250 V
Rated current: 16 A
Rated impulse voltage: 4 kV
Type of protection: IP40
Cable type: H05Z1Z1-F
Fire class: Eca
Cable color: black
Halogen-free: yes
Length: 5 m

Brand: Wieland Electric GmbH 
Type: GST18i3 K1 -S 15H 50GN07
Part No.: 92.297.5064.7

