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gesis® connection cable, male, free end, 5x 1.5 mm², 250/400 V, 16 A, Eca, length: 4 m, tomato red

System gesis® CLASSIC - assembled H05VV-F connection cable with protective ground, 5-pole, 1.5 mm², fire class Eca, male GST18i5, free end (ultrasonic welded), according IEC 61535, mechanical coding code 2, color coding tomato red.

Rated voltage: 250/400 V
Rated current: 16 A
Rated impulse voltage: 4 kV
Type of protection: IP40
Cable type: H05VV-F
Fire class: Eca
Cable color: black
Halogen-free: no
Length: 4 m

Brand: Wieland Electric GmbH 
Type: GST18i5 K1 -S 15E 40TR01
Part No.: 92.257.4004.0

