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gesis® connection cable, male, free end, 5x 1.0 mm², 250/400 V, 10 A, length: 8 m, white

System gesis® CLASSIC - assembled H05Z1Z1-F connection cable with protective ground, 5-pole, 1.0 mm², male GST18i5, free end (ultrasonic welded), according IEC 61535, mechanical coding code 1, color coding white.

Rated voltage: 250/400 V
Rated current: 10 A
Rated impulse voltage: 4 kV
Type of protection: IP40
Cable type: H05Z1Z1-F
Cable color: white
Halogen-free: yes
Length: 8 m

Brand: Wieland Electric GmbH 
Type: GST18i5 K1 -S 10H 80WS
Part No.: 92.256.8064.2

