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gesis® extension cable, female, male, 3x 1.5 mm², 250 V, 16 A, length: 5 m, black

System gesis® CLASSIC - assembled H05V2V2-F extension cable with protective ground, 3-pole, 1.5 mm², male GST18i3, female GST18i3, according IEC 61535, mechanical coding code 1, color coding black.

Rated voltage: 250 V
Rated current: 16 A
Rated impulse voltage: 4 kV
Type of protection: IP40
Cable type: H05V2V2-F
Continuous temperature: 90 °C
Cable color: black
Halogen-free: no
Length: 5 m

Brand: Wieland Electric GmbH 
Type: GST18i3 K1 BS 15W 50SW
Part No.: 92.232.5010.1

