
gesis® Snap-In, male, 5-pole, for panel mounting, 250/400 V, 20 A, may green

System gesis® CLASSIC - Installation connector according to IEC 61535 for permanent connection, male version, 5-pole, turned contacts with spring clamp connection, snapable in housing, with integrated locking, mechanical coding code 4, color coding may green.

Rated voltage: 250/400 V
Rated current: 20 A
Rated impulse voltage: 4 kV
Type of protection: IP40
Material thickness: 0.5 - 1.5 mm
Terminal cross-section, solid: 0.5 - 2.5 mm²
Terminal cross-section, stranded: 0.5 - 1.5 mm²
Housing material: Polyamide
Connections per pole: 2
Marking: 1, 2, PE, 3/N, 4
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: GST18i5 F S2 RV GN04
Part No.: 92.052.8058.0
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