
gesis® distribution block, 5-pole, 1 input, 3 outputs, 250/400 V, 20 A, white

System gesis® CLASSIC - Distribution block for installation connectors according to IEC 61535, H-shaped distribution block, 5-pole, turned contacts, 1 input, 3 outputs, with mounting option on distributor mounting plate 07.413.6853.1, with integrated locking, mechanical coding code 1, color coding white.

Rated voltage: 250/400 V
Rated current: 20 A
Rated impulse voltage: 4 kV
Type of protection: IP40
Housing material: Polyamide
Input: 1
Outputs: 3
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: GST18i5 V 3P1 V WS
Part No.: 92.050.6953.0
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