
gesis® Snap-In, male, 3-pole, for panel mounting, 250 V, 20 A, tomato red

System gesis® CLASSIC - Installation connector according to IEC 61535 for permanent connection, male version, 3-pole, turned contacts with spring clamp connection, snapable in housing, with integrated locking, mechanical coding code 2, color coding tomato red.

Rated voltage: 250 V
Rated current: 20 A
Rated impulse voltage: 4 kV
Type of protection: IP40
Material thickness: 0.5 - 1.5 mm
Terminal cross-section, solid: 0.5 - 2.5 mm²
Terminal cross-section, stranded: 0.5 - 1.5 mm²
Housing material: Polyamide
Connections per pole: 2
Marking: L, PE, N
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: GST18i3 F S2 RV TR01
Part No.: 92.032.9758.5
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