
RST® circular connector, IP66/68(3 m;2 h)/69, male, 5-pole, 250/400 V, 25 A, concrete gray

System RST® CLASSIC - Circular connector according to IEC 61535 for permanent installation with type of protection IP66/68(3 m;2 h)/69, male, 5-pole, turned contacts with screw connection compact housing with strain relief, field assembly, mechanical/color coding concrete gray/black.

Rated voltage: 250/400 V
Rated current: 25 A
Rated impulse voltage: 4 kV
Type of protection: up to IP66/68(3 m;2 h)/69
Terminal cross-section: 0.75 - 6.0 mm² (without ferrules)
Cable diameter: 13.0 - 18.0 mm (H05VV, H07RN-F)
Housing material: PA66, V2
Sealing material: NBR
Connections per pole: 1
Marking: L, N, PE, 1, 2
Halogen-free: yes

Brand: Wieland Electric GmbH  
Type: RST25I5S6S1 ZR3SV GR03
Part No.: 99.576.0000.7
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