
RST® distribution block, IP66/68(3 m; 2 h)/69, 2-pole, 1 input, 3 outputs, with mounting option, 250/400 V, 8 A, light blue

System RST® MICRO - distribution block for circular connector IP66/68(3 m; 2 h)/69, 1 input, 3 outputs, 2-pole, with mounting option on distributor mounting plate, mechanical/color coding light blue.

Rated voltage: 250/400 V
Rated current: 8 A
Rated impulse voltage: 4 kV
Type of protection: IP66/68(3 m; 2 h)/69
Housing material: PA66, V2
Sealing material: NBR
Input: 1
Outputs: 3
Halogen-free: yes
Dimension: 47x50.6x22.8 mm

Brand: Wieland Electric GmbH 
Type: RST08I2B 3P1 F VG BL
Part No.: 4L.020.0143.9
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