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RST® extension cable IP66/68(3 m; 2 h)/69, female, male, 5x 1.5 mm², power/signal, Eca, length: 1 m, turquoise blue

System RST® MINI - assembled H05VV-F extension cable IP66/68(3 m; 2 h)/69, 5-pole, 1.5 mm², fire class Eca, with locking, male RST16i5, female RST16i5, according to IEC 61535, mechanical/color coding turquoise blue.

Rated voltage: 250/400 V
Rated current: 16 A
Rated impulse voltage: 4 kV
Type of protection: IP66/68(3 m; 2 h)/69
Cable type: H05VV-F
Fire class: Eca
Cable color: black
Halogen-free: no
Length: 1 m

Brand: Wieland Electric GmbH  
Type: RST16I5K1BS 15PH 10TB
Part No.: 46.452.1000.6

