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RST® extension cable IP66/68(3 m; 2 h)/69, female, male, 5x 1.5 mm², 250/400 V, 16 A, length: 0.5 m, black

System RST® MINI - assembled H07RN-F extension cable IP66/68(3 m; 2 h)/69, 5-pole, 1.5 mm², with locking, male RST16i5, female RST16i5, according to IEC 61535, mechanical coding light gray/black, color coding black.

Rated voltage: 250/400 V
Rated current: 16 A
Rated impulse voltage: 4 kV
Type of protection: IP66/68(3 m; 2 h)/69
Cable type: H07RN-F
Cable color: black
Halogen-free: no
Length: 0.5 m

Brand: Wieland Electric GmbH  
Type: RST16I5K1BS 15 05SW
Part No.: 46.452.0530.1

