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RST® extension cable IP66/68(3 m; 2 h)/69, female, male, 2x 1.5 mm², low voltage, length: 1 m, signal brown

System RST® MINI - assembled H07RN-F extension cable IP66/68(3 m; 2 h)/69, 2-pole, 1.5 mm², with locking, male RST16i2, female RST16i2, according to IEC 61535, mechanical/color coding signal brown.

Rated voltage: 250 V
Rated current: 16 A
Rated impulse voltage: 4 kV
Type of protection: IP66/68(3 m; 2 h)/69
Cable type: H07RN-F
Cable color: black
Halogen-free: no
Length: 1 m

Brand: Wieland Electric GmbH  
Type: RST16I2K1BS 15L 10BR
Part No.: 46.422.1032.4

